|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **TEST INSTRUMENTS DETAILS** | | | | |
| Instrument | <Type> | Make | <Make> |  |
| Model | <Model> | Serial No | <SerialNumber> | |
| Calibrated on | <CalibratedOn> | Calibration Due On | <CalibratedDueOn> | |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **TEST RESULTS** | | | | | | |
| **S.No** | **Room Name/**  **AHU No** | **Condition** | **Particle Count per cubic meter per minute** | | | **Result** |
| **0.5 µ and above** | **1 µ and above** | **5 µ and above** |
| <sno> | <Name> | <Condition> | <pt-Average> | <1-Average> | <5-Average> | <Result> |
| <Condition> | <pt-Average> | <1-Average> | <5-Average> | <Result> |
| <Condition> | <pt-Average> | <1-Average> | <5-Average> | <Result> |
| **Results:** The above test results meet the specified requirement. | | | | | | |

**<QRCode>**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Result:** Systems recovering and meets the specified limits in <lmt> minute | | | | | | |
| **Reference:** This test carried out in accordance with ISO – 14644-3 | | | | | | |
| Maximum Permitted number of particles/m³ equal to or above | | | | | | |
| **Class** | **At rest** | | | **In Operation** | | |
| **≥ 0.5 µm** | **≥ 1 µm** | **≥ 5 µm** | **≥ 0.5 µm** | **≥ 1 µm** | **≥ 5 µm** |
| <O-ClassName> | <R-PointMicron> | <R-OneMicron> | <R-FiveMicron> | <O-PointMicron> | <O-OneMicron> | <O-FiveMicron> |